{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":55,"n_cols":12,"rows_kept":55,"cut":false,"hidden":false,"merged":[[2,0,2,1],[2,3,2,4],[2,7,2,8],[2,10,2,11]]}
[]
[]
["提升机&穿梭车",null,null,"输送线",null,null,null,"堆垛机",null,null,"拆叠盘机"]
[0,"设备空闲",null,0,"空闲",null,null,35,"取货后货叉无货",null,0,"空闲"]
[1,"运行中",null,1,"运行",null,null,36,"放货时货架有货-双伸",null,1,"执行中"]
[2,"动作完成",null,2,"完成",null,null,37,"放货后货叉有货",null,2,"完成"]
[30,"手动",null,30,"手动",null,null,38,"取货时货叉有货",null,30,"手动"]
[31,"急停",null,31,"急停",null,null,39,"放货时货叉无货",null,31,"急停"]
[32,"行走变频或伺服故障",null,32,"变频报警",null,null,40,"源地址错误",null,32,"提升电机报警"]
[33,"移载变频故障",null,33,"热继报警",null,null,41,"目地址错误",null,33,"夹抱电机报警"]
[34,"行走电机热继电器故障",null,34,"电辊筒报警",null,null,42,"高货低送报警",null,34,"超高报警  "]
[36,"车体输送货物超界 ",null,35,"输送超时报警",null,null,43,"货物超高",null,36,"上极限报警"]
[38,"行走条码阅读器报警",null,36,"升降超时报警",null,null,44,"货物超宽",null,37,"下极限报警"]
[39,"通讯故障(环rgv离线)",null,37,"顶升高低位异常",null,null,45,"货物超界",null,38,"伙伴报警"]
[40,"上位命令错误",null,45,"超界",null,null,46,"货叉不居中-单叉",null,39,"提升运行超时"]
[41,"行走停过界",null,46,"安全门打开",null,null,47,"叉左信号丢失",null,40,"货叉运行超时"]
[42,"取货时穿梭车上有货",null,47,"转台位置异常",null,null,48,"叉右信号丢失",null,41,"开关位置错误"]
[43,"送货穿梭车上无货",null,50,"顶升驱动报警",null,null,49,"叉左到位信号丢失",null,42,"高→中位运行超时"]
[44,"穿梭车接货超时",null,51,"跟随超时报警",null,null,50,"叉右到位信号丢失",null,43,"低→中位运行超时"]
[45,"穿梭车送货超时",null,52,"光栅报警",null,null,51,"货叉运行超时-双伸"]
[46,"行程后极限",null,53,"备用报警3",null,null,52,"取货时货叉提货超时"]
[47,"行程前极限",null,54,"货物类型未知",null,null,53,"放货时货叉放货超时"]
[48,"行走测距值未变",null,55,"货物类型与实际不匹配",null,null,60,"目标地址未设置"]
[49,"取货时对接输送机无货",{"$nulls":5},61,"行走测距故障"]
[50,"放货时对接输送机上有货",{"$nulls":5},62,"升降测距故障"]
[51,"送货时对接输送机未动作",{"$nulls":5},63,"行走停过界"]
[52,"货物不居中",{"$nulls":5},64,"升降停过界"]
[53,"地面输送机超界",{"$nulls":5},66,"升降时测距值未变"]
[54,"安全门打开",{"$nulls":5},67,"行走时测距值未变"]
[55,"激光防碰动作",{"$nulls":5},68,"升降目标值超限"]
[56,"输送机超时",{"$nulls":5},69,"行走目标值超限"]
[59,"上位机急停",{"$nulls":5},70,"升降速度异常"]
[60,"前安全触边报警",{"$nulls":5},71,"行走速度异常"]
[61,"后安全触边报警",{"$nulls":5},72,"升降未在正常范围值内"]
[62,"车间距离过小",{"$nulls":5},73,"行走未在正常范围值内"]
[63,"控制台手动",{"$nulls":5},74,"光通讯断"]
[64,"控制台急停",{"$nulls":5},75,"取货时站台未就绪"]
[65,"维修工位维修中",{"$nulls":5},76,"放货时站台未就绪"]
[66,"输送时提升超界",{"$nulls":5},78,"运动时切换模式"]
[72,"提升变频报警",{"$nulls":5},79,"行走校验错"]
[73,"输送变频报警",{"$nulls":5},80,"升降校验错"]
[75,"条码定位错误",{"$nulls":5},93,"行走运行超时"]
[76,"货物超界",{"$nulls":5},95,"取远端货时近端有货"]
[80,"命令错",{"$nulls":5},96,"放远端货时近端有货"]
[82,"取货时提升机有货",{"$nulls":5},97,"取货时托盘类型不符"]
[83,"放货时提升机无货",{"$nulls":5},98,"放货时托盘类型不符"]
[85,"松绳报警",{"$nulls":5},102,"安全门打开"]
[90,"替罪羊报警",{"$nulls":5},107,"左回叉时右超界"]
[91,"送货时输送机未动作",{"$nulls":5},108,"右回叉时左超界"]
[93,"分层超界报警",{"$nulls":5},109,"货叉码值超限"]
[102,"上极限",{"$nulls":5},110,"远叉码值超限"]
[103,"下极限",{"$nulls":5},111,"货叉编码器掉站"]
[104,"输送超时",{"$nulls":5},112,"远深货叉编码器掉站"]
[105,"提升超时",{"$nulls":5},114,"上位机急停"]
[{"$nulls":7},129,"载货台倾斜"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}